{"text_format":"5","workbook":"xls","n_sheets":1,"sheets":["TYRE LIST"],"props":{"creator":"SPIDOM","last_modified_by":"Vincenzo Ramadori","company":"HONDA ITALIA IND.LE S.p.A."},"not_rendered":{"images":1,"macros":1,"external_links":1,"defined_names":1,"comments":3},"notes":{"written":3,"chars":77},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"TYRE LIST","index":0,"n_rows":106,"n_cols":15,"rows_kept":106,"merged":[[0,7,0,10],[1,4,2,11],[2,1,2,3],[5,1,5,14],[6,1,6,4],[6,5,7,5],[6,6,6,7],[6,8,6,10],[6,11,6,12],[6,13,6,14],[14,1,16,1],[14,11,16,11],[14,12,16,12],[14,13,16,13],[14,14,16,14],[18,1,19,1],[18,11,19,11],[18,12,19,12],[18,13,19,13],[18,14,19,14],[26,1,28,1],[26,11,28,11],[26,12,28,12],[26,13,28,13],[26,14,28,14],[31,1,33,1],[31,11,33,11],[31,12,33,12],[31,13,33,13],[31,14,33,14],[35,2,36,2],[35,11,36,11],[35,12,36,12],[35,13,36,13],[35,14,36,14],[38,2,39,2],[40,2,43,2],[41,4,43,4],[41,11,43,11],[41,12,43,12],[41,13,43,13],[41,14,43,14],[44,1,45,1],[44,2,45,2],[46,1,47,1],[46,2,47,2],[46,11,47,11],[46,12,47,12],[46,13,47,13],[46,14,47,14],[51,1,53,1],[51,2,53,2],[51,11,53,11],[51,12,53,12],[51,13,53,13],[51,14,53,14],[59,11,61,11],[59,12,61,12],[59,13,61,13],[59,14,61,14],[63,2,66,2],[63,11,66,11],[63,12,66,12],[63,13,66,13],[63,14,66,14],[64,4,66,4],[67,11,68,11],[67,12,68,12],[67,13,68,13],[67,14,68,14],[69,2,71,2],[69,11,71,11],[69,12,71,12],[69,13,71,13],[69,14,71,14],[72,1,73,1],[72,2,73,2],[72,11,73,11],[72,12,73,12],[72,13,73,13],[72,14,73,14],[74,1,76,1],[74,2,76,2],[74,11,76,11],[74,12,76,12],[74,13,76,13],[74,14,76,14],[77,1,78,1],[77,2,78,2],[77,11,78,11],[77,12,78,12],[77,13,78,13],[77,14,78,14],[79,1,80,1],[79,2,80,2],[79,4,80,4],[79,11,80,11],[79,12,80,12],[79,13,80,13],[79,14,80,14],[83,1,84,1],[83,2,84,2],[85,2,89,2],[85,11,89,11],[85,12,89,12],[85,13,89,13],[85,14,89,14],[90,4,91,4],[90,11,91,11],[90,12,91,12],[90,13,91,13],[90,14,91,14],[93,2,94,2],[93,11,94,11],[93,12,94,12],[93,13,94,13],[93,14,94,14],[95,1,96,1],[95,2,96,2],[95,11,96,11],[95,12,96,12],[95,13,96,13],[95,14,96,14],[97,2,100,2],[97,4,100,4],[97,11,100,11],[97,12,100,12],[97,13,100,13],[97,14,100,14]],"headers":{"header":["","","Elenco Honda edizione settembre 2009"],"footer":["","","pagina di"]},"flags":["formulas_cached_only"]}
[]
[{"$nulls":4},"           TYRE LIST FOR                                        REPEATIBILITY OF TYRES"]
[null,"HONDA ITALIA INDUSTRIALE S.P.A"]
[]
[]
[]
[null,"HOMOLOGATION REFERENCE",{"$nulls":3},"MAX SPEED Km/h","RIM SIZE",null,"MAX PERMISSIBLE WEIGHT",null,null,"HOMOLOGATED TYRES",null,"ALTERNATIVE TYRES"]
[null,"VEHICLE TYPE","COMMERCIAL NAME","OMOLOGATION N°","YM",null,"FR","RR","TOT","FR AXLE","RR AXLE","TYRE FR","TYRE RR","TYRE FR","TYRE RR"]
[1,"CB1","CBX 1000","OM 18476",1978,223.6,"N.A.","N.A.",414,"N.A.","N.A.","3.50-V19 PRA","4.25-V18 PR4","100/90-19 57V","120/90-18 65V"]
[2,"CB 250N",null,"OM  19255",1979,128.5,"N.A.","N.A.",320,"N.A.","N.A.","3.60-S19 PR4","4.10-S18 PR4","100/90-19 57H","110/90-18 61H"]
[3,"CB 250T",null,"OM 18164",1978,122.9,"N.A.","N.A.",320,"N.A.","N.A.","3.60-S19 PR4","4.10-S18 PR4","100/90-19 57H","110/90-18 61H"]
[4,"CB 350",null,"R.T. 2276",1972,130,"N.A.","N.A.",323,"N.A.","N.A.","3.00 X 18 PR4","3.50 X 18 PRA","90/90-18 51H","110/90-18 61H"]
[5,"CB 350F",null,"R.T. 2374",1973,151.3,"N.A.","N.A.",327,"N.A.","N.A.","3.00 X 18 PR4","3.50 X 18 PRA","90/90-18 51H","110/90-18 61H"]
[6,"CB 400F",null,"OM 14677",1975,148.2,"N.A.","N.A.",323,"N.A.","N.A.","3.00 X 18 PR4","3.50 X 18 PRA","90/90-18 51H","110/90-18 61H"]
[7,"CB 400N",null,"OM 18477",1978,153.8,"N.A.","N.A.",329,"N.A.","N.A.","3.60-S19 PR4","4.10-S18 PR4","100/90-19 57H","110/90-18 61H"]
[8,null,null,"OM 18477B",1981,153.8,"N.A.","N.A.",329,"N.A.","N.A."]
[9,null,null,"OM 18477C",1982,153.8,"N.A.","N.A.",329,"N.A.","N.A."]
[10,"CB 400T",null,"OM 17543",1977,154.8,"N.A.","N.A.",320,"N.A.","N.A.","3.60-S19 PR4","4.10-S18 PR4","100/90-19 57H","110/90-18 61H"]
[11,"CB 450 ",null,"R.T. 1512",1970,135.85,"N.A.","N.A.",320,"N.A.","N.A.","3.25 X S19 PR4","3.50 X 18 PR4","100/90-19 57H","110/90-18 61H"]
[12,null,null,"R.T. 2239",1972,135.85,"N.A.","N.A.",320,"N.A.","N.A."]
[13,"CB 500",null,"R.T. 2419",1973,146.7,"N.A.","N.A.",343.5,"N.A.","N.A.","3.25 X S19 PR4","3.50 X 18 PR4","100/90-19 57H","110/90-18 61H"]
[14,"CB 500","FOUR","OM 15745",1976,146.7,"N.A.","N.A.",343.5,"N.A.","N.A.","3.25 X S19 PR4","3.50 X 18 PR4","100/90-19 57H","110/90-18 61H"]
[15,"CB 500K",null,"OM 16663",1977,168.7,"N.A.","N.A.",352,"N.A.","N.A.","3.25 X S19 PR4","3.75-S18 PR4","100/90-19 57H","110/90-18 61H"]
[16,"CB 500T",null,"OM 14678",1975,164.9,"N.A.","N.A.",348,"N.A.","N.A.","3.25 X S19 PR4","3.75-S18 PR4","100/90-19 57H","110/90-18 61H"]
[17,"CB 550F",null,"OM 15124",1975,155.8,"N.A.","N.A.",344,"N.A.","N.A.","3.25 X S19 PR4","3.75-S18 PR4","100/90-19 57H","110/90-18 61H"]
[18,"CB 550K",null,"OM 16664",1977,169.4,"N.A.","N.A.",352,"N.A.","N.A.","3.25 X S19 PR4","3.75-S18 PR4","100/90-19 57H","110/90-18 61H"]
[19,"CB 750",null,"R.T. 1523",1970,161,"N.A.","N.A.",373,"N.A.","N.A.","3.25 X S19 PR4","4.00-S18 PR4","100/90-19 57H","120/90-18 65H"]
[20,null,null,"R.T. 2238",1972,161,"N.A.","N.A.",373,"N.A.","N.A."]
[21,null,"Senior","R.T. 2268",1972,188.27,"N.A.","N.A.",305,"N.A.","N.A."]
[22,"CB 750F",null,"OM 15123",1975,176.9,"N.A.","N.A.",382.5,"N.A.","N.A.","3.25 X H19 PR4","4.00-H18 PR4","100/90-19 57H","120/90-18 65H"]
[23,"CB 750K",null,"OM 16662",1977,186,"N.A.","N.A.",390,"N.A.","N.A.","3.50 H19 PR4","4.50-H17PR4","110/90-19 57H","130/90-17 68V"]
[24,"CX 500",null,"OM 18072",1978,164.3,"N.A.","N.A.",360,"N.A.","N.A.","3.25 X S19 PR4","3.75-S18 PR4","100/90-19 57H","110/90-18 61H"]
[25,null,null,"OM 18072B",1978,164.3,"N.A.","N.A.",360,"N.A.","N.A."]
[26,null,null,"OM 18072C",1981,164.3,"N.A.","N.A.",360,"N.A.","N.A."]
[27,"GL-1 - ED",null,"OM 15048",1975,180,"N.A.","N.A.",430,"N.A.","N.A.","3.50 H19 PR4","4.50-H17A PR4","100/90-19 57H","130/90-17 68V"]
[28,"JD10","CRM 125R","OM 52852",1989,125,"1,6X21","2,15X18",270,"N.A.","N.A.","3.00-21 51P","4.60-18 63P","90/90-21 54R","120/90-18 65 H"]
[29,"JD10-A",null,"OM 52852 EST01",1995,105,"1,6X21","2,15X18",270,"N.A.","N.A."]
[30,"JD12","NX 125","OM 52779",1989,110,"1,6X21","2,15X17",270,"N.A.","N.A.","3.00-21 51R","4.60-17 62R","90/90-21 54R","120/90-17 64S"]
[31,"MC13","CMX 250 C","OM 54103",1996,115,"1,85X18","--",332,107,230,"3.00-18 47P","REP.130/90-15 M/C 66P",{"v":"90/90-18 51H","$note":[{"t":"SPIDOM:\nMICHELIN 2004 PAG 14"}]},"REP.130/90-15 M/C 66P"]
[32,"MC32",null,"OM 54253",1997,115,"1,85X18","--",332,110,232,"3.00-18 47P","REP.130/90-15 M/C 66P",{"v":"90/90-18 51H","$note":[{"t":"SPIDOM:\nMICHELIN 2004 PAG 14"}]},"REP.130/90-15 M/C 66P"]
[33,"MD06","XL 200R","OM 51290",1983,110,"N.A.","N.A.",264,"N.A.","N.A.","2.75-21 K550","4.10-18 K550","80/90-21 48H","110/90-18 61H"]
[34,"MD06-A",null,"OM 51290EST01",1984,108,"N.A.","N.A.",273,"N.A.","N.A.","2.75-21 45P","4.10-18 60P","80/90-2148H","110/90-18 61H"]
[35,"MD06-B",null,"OM 51290EST02",null,108,"N.A.","N.A.",273,"N.A.","N.A."]
[36,"MD06-C",null,"OM 51290EST03",null,108,"N.A.","N.A.",273,"N.A.","N.A."]
[37,"MF02","CN 250          ","OM 52515",1988,110,"2,50X12","--",308,"N.A.","N.A.","4.00-12 4PR","REP.120/90-10 65J","110/100-12 67J","REP.120/90-10 65J"]
[38,null,null,"OM 52515B",1991,110,"2,50X12","--",308,"N.A.","N.A.","REP.110/100-12 67J","REP.120/90-10 65J","110/100-12 67J","REP.120/90-10 65J"]
[39,"NC01","CM 400T","OM 50126",1980,152.2,"N.A.","N.A.",322,"N.A.","N.A.","3.50-S18 PR4","4.60-S16 PR4","110/90-18 61S","120/90 16 63S"]
[40,null,null,"OM 50126B",1981,152.2,"N.A.","N.A.",322,"N.A.","N.A."]
[41,"NC07","CBX 400F/FII","OM 50689",1982,167.16,"N.A.","N.A.",343,"N.A.","N.A.","3.60-H18 PR4","4.10-H18 PR4","100/90-18 61H","110/90-18 61H"]
[43,"ND01","XL400 R","OM 51694",1985,130,"N.A.","N.A.",287,"N.A.","N.A.","3,00/21 4PR","4,60 -17 4PR","90/90-21 54S","130/70 17 62V"]
[43,"ND03","XL350 R","OM 51799",1985,130,"N.A.","N.A.",287,"N.A.","N.A.","3,00/21 4PR","4,60 -17 4PR","90/90-21 54P","120/90 17 64P"]
[44,"PC01","CX 500C","OM 50125",1980,160.7,"N.A.","N.A.",361,"N.A.","N.A.","3.50-S19 PR4 (*)si allega copia lettera ministeriale per correzione Prot.4477/MOT2/L/175","REP.130/90-16 67S","110/90-19 57H","REP.130/90-16 67S"]
[45,null,null,"OM 50125B",1981,160.7,"N.A.","N.A.",361,"N.A.","N.A."]
[46,null,null,"OM 50125C",1981,160.7,"N.A.","N.A.",361,"N.A.","N.A."]
[47,"PC02","GL 500","OM 50688",1982,153.78,"N.A.","N.A.",385,"N.A.","N.A.","3.50 S19 PR4","REP. 130/90-16 67S","110/90-19 61 H","REP. 130/90-16 67S"]
[48,"PC03","CX 500TURBO","OM 50690",1982,198.2,"N.A.","N.A.",400,"N.A.","N.A.","3.50-V18 PR4","REP.120/90-17V","110/90-18 61V","REP. 120/90-17V"]
[49,"PC04","CBX 550","OM 50717",1982,199.55,"N.A.","N.A.",346,"N.A.","N.A.","3.60-H18 PR4","4.10-H18 PR4","100/90-18 56H","110/90-18 61H"]
[50,"PC07","FT 500","OM 50716",1982,144.49,"N.A.","N.A.",311,"N.A.","N.A.","3.50-S19 PR4","4.25-S18 PR4","100/90-19 56S","120/90-18 65S"]
[51,"PC08","VT 500C","OM 51042",1983,164.346,"N.A.","N.A.",333,"N.A.","N.A.","3.50-S18 PR4","REP. 130/90-16  67S","110/90-18 61H","REP. 130/90-16  67S"]
[54,"PD01","XL 500S","OM 19509",1979,136.3,"N.A.","N.A.",283,93,220,"3.00-23 PR4","4.60-18 PR4","90/90-23","130/80-18 66S"]
[55,"PD01","XL 500S","OM 19509B",1980,136.3,"N.A.","N.A.",283,93,220]
[56,"PD01-52","XL 500S","OM 50341",1981,136.3,"N.A.","N.A.",283,93,220]
[57,"PD02","XL 500R","OM 50687",1982,129.4,"N.A.","N.A.",288,"N.A.","N.A.","3.00-21 PR4","4.60-17 PR4","90/90-21 54S","120/80-17"]
[58,"PD03","XL 600R","OM 51127",1983,152.769,"N.A.","N.A.",286,"N.A.","N.A.","3.00-21 4PR","5.10-17 4PR","90/90-2154S","120/90-17 64S                                "]
[59,"PD03-A",null,"OM 51127 EST01",1984,150,"N.A.","N.A.",298,"N.A.","N.A."]
[60,"PD03-B",null,"OM 51127 EST02",null,150,"N.A.","N.A.",298,"N.A.","N.A."]
[61,"PD03-C",null,"OM 51127 EST03",null,150,"N.A.","N.A.",298,"N.A.","N.A."]
[62,"PD04","XL 600LM/RM","OM 51802",1985,150,"N.A.","N.A.",322,"N.A.","N.A.","3.00-21 4PR","5.10-17 4PR","90/90-21 54S","140/80-17 69S  "]
[63,"PD04-A","XL 600LM","OM 51802EST01",1986,150,"N.A.","N.A.",310,"N.A.","N.A."]
[64,"RC01","CB 750K","OM 19038",1979,191.5,"N.A.","N.A.",393,"N.A.","N.A.","3.25-H19 PR4","4.00 H18 4PR","110/90-19 57H","120/90-18 65H"]
[65,"RC01-A",null,"OM 19038EST 20063",1980,198.9,"N.A.","N.A.",393,"N.A.","N.A."]
[65,"RC01-A",null,"OM 19038EST 20063B",1981,198.9,"N.A.","N.A.",393,"N.A.","N.A."]
[66,"RC03","CB 650K","OM 19040",1979,177.3,"N.A.","N.A.",587,"N.A.","N.A.","3.25-H19 PR4","3.75-H18 PR4","100/90-19 57H","110/90-18 61H"]
[67,null,null,"OM 19040B",1981,177.3,"N.A.","N.A.",287,"N.A.","N.A."]
[68,"RC04","CB 750F","OM 50166",1980,195.1,"N.A.","N.A.",391,"N.A.","N.A.","3.25-H19 PR4","4.00-H18 PR4","100/90-19 57H","120/90-18 65H"]
[69,null,null,"OM 50166B",1981,195.1,"N.A.","N.A.",391,"N.A.","N.A."]
[70,null,null,"OM 50166C",1982,195.1,"N.A.","N.A.",391,"N.A.","N.A."]
[71,"RC05","CB 650C","OM 50152",1980,169.4,"N.A.","N.A.",361,"N.A.","N.A.","3.50 S19 PR4","REP.130/90-16 67S","110/90-19 57H","REP.130/90-16 67S"]
[72,null,null,"OM 50152B",1981,169.4,"N.A.","N.A.",361,"N.A.","N.A."]
[73,"RC07-A","VF 750S","OM 50747 EST01",1983,214.86,"N.A.","N.A.",382,"N.A.","N.A.","100/90-18 61H","130/90-17 68H",{"v":"110/90-18 61H","$note":[{"t":"SPIDOM:\nMICHELIN 2004"}]},"130/90-17 68V"]
[74,null,null,"OM 50747 EST01B",null,214.86,"N.A.","N.A.",382,"N.A.","N.A."]
[75,"RC08","CB 650C","OM 50656",1982,167.4,"N.A.","N.A.",359,"N.A.","N.A.","3.50 S19 PR4","REP.130/90-16 67S","100/90-19 57H","REP.130/90-16 67S"]
[76,"RC10","GL 650II","OM 50908",1982,173.9,"N.A.","N.A.",417,"N.A.","N.A.","3.50 H19 PR4","130/90-16 67H","100/90-19 57H","130/90-16 67H"]
[78,"SC01","CB 900E","OM 19346",1979,194,"N.A.","N.A.",395,"N.A.","N.A.","3.25-V19 PR4","4.00-V18 PR4","100/90-19 57V","120/90-18 65V"]
[79,null,null,"OM 19346B",1979,194,"N.A.","N.A.",396,"N.A.","N.A.","3.25-V19 PR4","4.00-V18 PR4","100/90-19 57V","120/90-18 65V"]
[80,"SC02","GL 1100","OM 50141",1980,191.5,"N.A.","N.A.",500,185,315,"REP.110/90-19 62H","130/90-17 68H","REP.110/90-19 62H","130/90-17 68V"]
[81,"SC02-A",null,"OM 50141EST01",1981,191.5,"N.A.","N.A.",494,"N.A.","N.A."]
[81,"SC02-B",null,"OM 50141EST02",1982,190.5,"N.A.","N.A.",494,"N.A.","N.A."]
[81,"SC02-C",null,"OM 50141EST03",1982,183.7,"N.A.","N.A.",494,"N.A.","N.A."]
[81,"SC02-D",null,"OM 50141EST04",1982,233.34,"N.A.","N.A.",494,"N.A.","N.A."]
[82,"SC03","CBX 1000","OM 50009",1980,216.9,"N.A.","N.A.",410,"N.A.","N.A.","3.50 V19 PR4","4.25 V18 PR4","100/90-19 57V","120/90-18 65V"]
[83,"SC03/J","CBX 1000","OM 50009EST01",null,209.9,"N.A.","N.A.",410,"N.A.","N.A."]
[84,"SC06","CBX","OM 50465",1981,204.5,"N.A.","N.A.",466,188,300,"3.50 V19 PR4","130/90-V18","100/90-19 57V","130/80-18 66V"]
[86,"TC01","NS 125F/R","OM 51747",1985,145,"N.A.","N.A.",264,"N.A.","N.A.","3.25-16 48P","3.50-18 62P","100/90-16 48P","110/90-18 61V"]
[87,"TC01-A",null,"OM 51747B",1986,145,"N.A.","N.A.",264,"N.A.","N.A."]
[88,"TC02","MTX 125R","OM 51933",1985,125,"N.A.","N.A.",270,"N.A.","N.A.","3.00-21 51R","4.60-18 63R","90/90-21 54R","120/90-18 65R"]
[89,null,null,"OM 51933B",1987,125,"N.A.","N.A.",270,"N.A.","N.A."]
[90,"TD01","XL 125 R/PD","OM 51452",1984,105,"N.A.","N.A.",264,"N.A.","N.A.","2.75-21 45P","4.10-18 60P","80/90-21 48P ","110/90-18 61P"]
[91,"TD01-A",null,"OM 51452EST01",null,102,"N.A.","N.A.",272,"N.A.","N.A."]
[92,"TD01-B",null,"OM 51452EST02",null,102,"N.A.","N.A.",272,"N.A.","N.A."]
[93,"TD01-C",null,"OM 51452EST03",null,102,"N.A.","N.A.",272,"N.A.","N.A."]
[94,"XL 125S","XL 125S","OM 50659",1982,99.5,"N.A.","N.A.",253,"N.A.","N.A.","2.75-21 PR4","4.10-18 PR4","80/90-21 48P ","110/90-18 61P"]
[]
[]
[]
[null,"N.A. = NOT AVAILABLE DATA"]